{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["Accueil","Calepinage","Bon de commande","BD","Schémas"],"not_rendered":{"charts":0,"images":64,"macros":1,"external_links":0,"defined_names":3,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Accueil","index":0,"n_rows":46,"n_cols":13,"rows_kept":46,"cut":false,"hidden":false,"merged":[[2,2,2,12],[3,2,3,12],[6,3,8,12],[39,2,40,3]]}
["                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      "]
[]
[null,null,"BIENVENUE DANS L'OUTIL DE DIMENSIONNEMENT ET COMMANDE "]
[null,null,"DU GSE INTEGRATION IN-ROOF SYSTEM"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Français"]
[null,null,null,"Vous trouverez à travers cette application l'outil qui vous permettra de calculer et de dimensionner vos commandes"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,","]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"Groupe Solution Energie"]
[null,null,null,null,null,null,null,"155 - 159 Rue du docteur Bauer - 93400 Saint Ouen"]
[null,null,null,null,null,null,null,"Tel: 01 49 48 14 51 - contact@gseintegration.com - www.gseintegration.com"]

{"sheet":"Calepinage","index":1,"n_rows":22,"n_cols":60,"rows_kept":22,"cut":false,"hidden":false,"merged":[[1,2,1,3],[1,5,1,6],[2,27,2,29],[29,32,29,36],[29,45,29,48],[30,32,30,36],[30,45,30,48],[32,49,32,51],[32,57,32,58],[3,27,3,29],[3,31,3,33],[3,35,3,37],[3,39,3,41],[2,31,2,33],[2,35,2,37],[2,39,2,41],[4,17,4,24],[5,3,5,4],[5,8,5,15],[5,17,5,18],[5,20,5,21],[5,23,5,24],[32,80,33,90],[33,47,33,49],[33,50,33,52],[33,53,33,55],[33,56,33,58],[34,47,34,49],[34,50,34,52],[34,53,34,55],[34,56,34,58],[37,47,37,49],[37,50,37,52],[37,53,37,55],[37,56,37,58],[37,82,37,85],[37,87,37,90],[35,47,35,49],[35,50,35,52],[35,53,35,55],[35,56,35,58],[36,47,36,49],[36,50,36,52],[36,53,36,55],[36,56,36,58],[39,47,39,49],[39,50,39,52],[39,53,39,55],[39,56,39,58],[39,87,39,88],[39,89,39,90],[38,47,38,49],[38,50,38,52],[38,53,38,55],[38,56,38,58],[38,87,38,88],[38,89,38,90],[41,47,41,49],[41,50,41,52],[41,53,41,55],[41,56,41,58],[41,87,41,88],[41,89,41,90],[40,47,40,49],[40,50,40,52],[40,53,40,55],[40,56,40,58],[40,87,40,88],[40,89,40,90],[43,47,43,49],[43,50,43,52],[43,53,43,55],[43,56,43,58],[43,87,43,88],[43,89,43,90],[42,47,42,49],[42,50,42,52],[42,53,42,55],[42,56,42,58],[42,87,42,88],[42,89,42,90],[45,50,45,52],[45,53,45,55],[45,56,45,58],[45,87,45,88],[45,89,45,90],[46,50,46,52],[46,53,46,55],[46,56,46,58],[44,47,44,49],[44,50,44,52],[44,53,44,55],[44,56,44,58],[44,87,44,88],[44,89,44,90],[47,50,47,52],[47,53,47,55],[47,56,47,58],[47,84,47,87],[48,50,48,52],[48,53,48,55],[48,56,48,58],[48,80,48,83],[48,84,48,87],[51,84,51,87],[49,50,49,52],[49,53,49,55],[49,80,49,83],[49,84,49,87],[50,50,50,52],[50,53,50,55],[50,80,50,83],[50,84,50,87]]}
[]
[]
[]
[]
[]
[]
[null,null,1,2,3,4,5,6,7,8,9,10,11,12,13,14,null,null,null,null,null,null,null,null,null,24,25,26,27,28,29,30,31,32,33,34,35,36,37,38,39,40,41,42,43,44,45,46,47,48,49,50,51,52,53,54,55,56,57,58]
[]
[1]
[2,null,"0.992 m","1.984 m","2.976 m","3.968 m","4.96 m","5.952 m","6.944 m","7.936 m","8.928 m","9.92 m","10.912 m","11.904 m","12.896 m","13.888 m","14.88 m"]
[3,"1.64 m"]
[4,"3.28 m"]
[5,"4.92 m"]
[6,"6.56 m"]
[7]
[8]
[9]
[10]
[11]
[12]
[13]
[14]

{"sheet":"Bon de commande","index":2,"n_rows":38,"n_cols":10,"rows_kept":38,"cut":false,"hidden":false,"merged":[[37,1,37,9],[38,1,38,9],[39,1,39,9],[33,1,33,9],[34,1,34,9],[35,1,35,9],[1,12,2,12],[1,16,2,16],[4,1,4,2],[1,1,1,9],[3,6,3,9],[4,6,4,9],[31,1,31,4],[18,2,18,4],[19,2,19,4],[20,2,20,4],[21,2,21,4],[24,2,24,4],[28,1,28,4],[29,1,29,4],[30,1,30,4],[26,1,26,4],[25,2,25,4],[5,6,5,9],[6,6,6,9],[7,6,7,9],[22,2,22,4],[23,2,23,4],[16,2,16,4],[17,2,17,4],[5,1,5,2],[14,2,14,4],[15,2,15,4],[9,1,9,4],[10,2,10,4],[11,2,11,4],[12,2,12,4],[13,2,13,4]]}
[]
[null,"PV Plant 1"]
[]
[null,null,null,null,null,null,"CONTACT DETAILS"]
[null,"DATE"]
[null,{"$f":" TODAY()","v":"2018-01-19"}]
[]
[]
[]
[null,"KIT GSE INTEGRATION PORTRAIT",null,null,null,"REFERENCES","NUMBER OF PIECES","UNIT PRICE (EXCL TAX)","UNIT PRICE DISCOUNTED","TOTAL"]
[null,null,"GSE Plate Portrait standard 1640 / 992",null,null,"PPORT 1640 / 992",15,34.15,22.197500000000002,{"$f":" G11 * I11","v":332.96250000000003}]
[null,null,"Universal Lateral Flashing Standard BLACK",null,null,"ALUN",12,11.19,7.2735000000000003,{"$f":" G12 * I12","v":87.282000000000011}]
[null,null,"Top Right Corner Flashing BLACK",null,null,"COINDNOIR2014_15",0,16.07,10.445500000000001,0]
[null,null,"Top Left Corner Flashing BLACK",null,null,"COINGNOIR2014_15",0,16.07,10.445500000000001,0]
[null,null,"Top Centre Flashing (LG 1.50 m) BLACK",null,null,"AFCUNL1500",0,20.239999999999998,13.155999999999999,0]
[null,null,"Corner Piece (To Join Module to Top Centre Flashings) BLACK",null,null,"CORNIERELAQUEB",0,4.17,2.7105000000000001,0]
[null,null,"Pop Rivet (4-Fixations Rivet for Top Centre Flashing)",null,null,"RIVETPOP",0,0.05,3.2500000000000001E-2,0]
[null,null,"Junction For Top Flashing BLACK",null,null,"AFJUNL375",0,5.36,3.4840000000000004,0]
[null,null,"Selt-Trapping Screw + GSE Washer Silver ( 6 per Frame)",null,null,"VIS2014A",90,0.27,0.17550000000000002,15.795000000000002]
[null,null,"Selt-Trapping Screw + GSE Washer Black to fix Clamp BLACK",null,null,"VIS2014N",36,0.27,0.17550000000000002,6.3180000000000005]
[null,null,"Cale EPDM Cell 5 mm",null,null,"CALE_EPDM_CELL",36,0.08,5.2000000000000005E-2,1.8720000000000001]
[null,null,"Reinforced Double Clamp H16 BLACK",null,null,"EDH162014N ",24,1.4,0.90999999999999992,21.839999999999996]
[null,null,"Reinforced Single Clamp H16 BLACK",null,null,"ESH162014N ",12,1.21,0.78649999999999998,9.4379999999999988]
[null,null,"Batch of 4 Reinforcement GSE Wedges L and R for Single Clamps",null,null,"CALE_GAUCHE / CALE_DROIT",3,0.98,0.63700000000000001,1.911]
[null,null,"GSE Flashing Hook",null,null,"CROCHET",32,0.6,0.39,12.48]
[null,null,"Pre-Compressed Seal Roll - 20 x 40 mm (5.5 m roll)",null,null,"JOINT_PRE_CONTRAIN",0,6.33,4.1145000000000005,0]
[null,"TOTAL",null,null,null,null,null,null,{"$f":"SUM(I11:I26)","v":76.986000000000018},{"$f":" SUM(J11:J26)","v":489.89850000000001}]
[]
[null,"OPTIONS"]
[null,"ROOFLEX Waterproof Strip (5 m roll)",null,null,null,"BANDE_FLEXALU",0,"m"]
[null,"Roof-Underlay Screen (75 m² roll)",null,null,null,"ECRAN_SOUS_TOITURE ",30,"m²"]
[null,"NB: Price available from your usual contact."]
[]
[null,"DESIRED SHIPPING DATE"]
[]
[]
[]
[null,"ADDRESS / CONTACT / COMMENTS"]

{"sheet":"BD","index":3,"n_rows":124,"n_cols":26,"rows_kept":124,"cut":false,"hidden":false,"merged":[[13,6,13,8],[0,7,0,10],[0,11,0,12],[0,15,0,18],[0,19,0,20],[12,6,12,10],[22,15,22,18],[14,6,14,8],[14,14,15,20],[15,0,15,1],[15,6,15,8],[16,6,16,8],[17,6,17,8],[18,6,18,8],[18,15,18,20],[19,15,19,18],[20,15,20,18],[21,15,21,18],[29,0,29,1],[29,15,29,18],[30,15,30,18],[23,15,23,18],[24,15,24,18],[25,15,25,18],[26,15,26,18],[27,15,27,18],[28,15,28,18]]}
["Epaisseur Module PV","ID",null,"Plaque Ref.","largeur mi-ondes",null,"Dénomination","Tolérances dimensionnelles",null,null,null,"Dimensions de référence de la plaque GSE Portrait",null,null,"Dénomination","Tolérances dimensionnelles",null,null,null,"Dimensions de référence de la plaque GSE Paysage",null,null,"Variable","Français","English","Deutsch"]
[31,"H16",null,"1640 / 992",1028,null,"PLAQUE","HAUTEUR MINIMUM","HAUTEUR MAXIMUM","LARGEUR MINIMUM","LARGEUR MAXIMUM","Hauteur ref","Larg ref",null,"PLAQUE","HAUTEUR MINIMUM","HAUTEUR MAXIMUM","LARGEUR MINIMUM","LARGEUR MAXIMUM","Hauteur ref","Larg ref",null,"HomeT1","BIENVENUE DANS L'OUTIL DE DIMENSIONNEMENT ET COMMANDE ","WELCOME TO THE SIZING AND CONTROL TOOL ","WILLKOMMEN BEIM AUSLEGUNGS- UND BESTELLTOOL "]
[32,"H16",null,"1650 / 992",1028,null,"1559 / 1046",1535,1615,1037,1047,1559,1046,null,"1559 / 1046",1042,1122,1551,1560,1046,1559,null,"HomeT2","DU GSE INTEGRATION IN-ROOF SYSTEM","OF GSE INTEGRATION IN-ROOF SYSTEM","FÜR DAS GSE INTEGRATION IN-ROOF SYSTEM"]
[33,"H16",null,"1660 / 992",1028,null,"1575 / 1053",1535,1615,1044,1054,1575,1053,null,"1575 / 1082",1042,1122,1567,1576,1082,1575,null,"HomeT3","Vous trouverez à travers cette application l'outil qui vous permettra de calculer et de dimensionner vos commandes","You will find through this application the tool that will allow you to calculate and size your orders","Mit dieser Anwendung erhalten Sie ein Werkzeug, das es Ihnen erlaubt, Ihre Aufträge auszulegen und zu berechnen."]
[35,"H16",null,"1670 / 992",1028,null,"1575 / 1082",1535,1615,1073,1083,1575,1082,null,"1580 / 808",768,848,1572,1581,808,1580,null,"Dim","Dimensionner","Size","Auslegen"]
[38,"H19",null,"1675 / 992",1028,null,"1580 / 808",1540,1620,798,809,1580,808,null,"1640 / 992",952,1032,1632,1641,992,1640,null,"RefCmpPV","Référence du champ PV","Reference of the PV Plant","PV-Modulfeldreferenz"]
[39,"H21",null,"1680 / 992",1028,null,"1640 / 992",1600,1680,983,993,1640,992,null,"1650 / 992 ",952,1032,1642,1651,992,1650,null,"DimToit","Dimensions du toit","Roof Dimensions","Dachabmessungen"]
[40,"H21",null,"1640 / 1001",1038,null,"1640 / 1001",1600,1680,992,1002,1640,1001,null,"1660 / 992",952,1032,1652,1661,992,1660,null,"Calepinage","Calepinage","Layout","Lattenplan"]
[42,"H23",null,"1650 / 1001",1038,null,"1640 / 1001 P33",1600,1680,992,1002,1640,1001,null,"1670 / 992",952,1032,1662,1671,992,1670,null,"DimMod","Dimension du module","Module Dimensions","Modulabmessungen"]
[43,"H23",null,"1660 / 1001",1038,null,"1686 / 1016",1646,1726,1007,1017,1686,1016,null,"1675 / 992 P33",952,1032,1667,1676,992,1675,null,"Long","Longueur","Length","Länge"]
[45,"H27",null,"1670 / 1001",1038,null,null,null,null,null,null,null,null,null,"1680 / 992",952,1032,1672,1681,992,1680,null,"Ramp","Rampant","Roof Rake","Länge der Dachschräge"]
[46,"H27",null,"1675 / 1001",1038,null,null,null,null,null,null,null,null,null,"1686 / 1016",976,1056,1677,1687,1016,1686,null,"Haut","Hauteur","Height","Höhe"]
[50,"H31",null,"1680 / 1001",1038,null,"Shémas Plaques Portrait",null,null,null,null,null,null,null,"1700 / 1016",976,1056,1691,1701,1016,1700,null,"Larg","Largeur","Width","Breite"]
[null,null,null,"1580 / 808",844,null,"Références Plaques",null,null,"ID Plan 4 Etriers","ID Plan 6 Etriers",null,null,null,null,null,null,null,null,null,null,null,"Epai","Epaisseur","Thickness","Dicke"]
[null,null,null,"1559 / 1046",1082,null,"1559 / 1046 - 1575 / 1053 - 1575 / 1082",null,null,"Port_Plan11","Port_Plan12",null,null,null,"In the processing, as the height is considered to be the longest dimension, the width is inverted with the height",null,null,null,null,null,null,null,"CalPort","Calepinage portrait","Portrait Layout","Lattenplan für hochkant-Montage"]
["Liste de références \"Etriers doubles\"",null,null,"1575 / 1082",1118,null,"1580 / 808",null,null,"Port_Plan21","Port_Plan22",null,null,null,null,null,null,null,null,null,null,null,"CalPays","Calepinage paysage","Landscape Layout","Lattenplan für Querformat-Montage"]
["Etrier Double Renforcé H16 NOIR","EDH162014N ",null,"1575 / 1053",1089.5,null,"1640 / 992 - 1640 / 1001",null,null,"Port_Plan31","Port_Plan32",null,null,null,null,null,null,null,null,null,null,null,"CorPlakGSE","Plaque GSE correspondante","Corresponding GSE Plate","Entsprechende GSE-Wanne"]
["Etrier Double Renforcé H19 NOIR","EDH192014N ",null,null,null,null,null,null,null,"Port_Plan41","Port_Plan42",null,null,null,null,null,null,null,null,null,null,null,"FeatCmpPV","Caractéristiques de l'installation de champ PV","Characteristics of the PV Plant Installation","Eigenschaften der Installation des Modulfeldes"]
["Etrier Double Renforcé H21 NOIR","EDH212014N ",null,null,null,null,null,null,null,"Port_Plan51","Port_Plan52",null,null,null,null,"Shémas Plaques Paysage",null,null,null,null,null,null,"TypeCov","Type de couverture","Cover Type","Art der Dachbedeckung"]
["Etrier Double Renforcé H23 NOIR","EDH232014N",null,null,null,null,null,null,null,null,null,null,null,null,null,"Références Plaques",null,null,null,"ID Plan 4 Etriers","ID Plan 6 Etriers",null,"Ardoise","Ardoise","Slate","Schiefer"]
["Etrier Double Renforcé H27 NOIR","EDH272014N ",null,null,null,null,null,null,null,null,null,null,null,null,null,"1580 / 808",null,null,null,"Pays_Plan11","Pays_Plan12",null,"TuileC","Tuile canal","Curved Tiles","Kanalziegel"]
["Etrier Double Renforcé H31 NOIR","EDH312014N ",null,null,null,null,null,null,null,null,null,null,null,null,null,"1640 / 992 - 1650 / 992 - 1660 / 992 - 1670 / 992 - 1675 / 992 - 1680 / 992",null,null,null,"Pays_Plan21","Pays_Plan22",null,"Tuile","Tuile","Tiles","Ziegel"]
["Etrier Double Renforcé H16 ALU","EDH162014ALU",null,null,null,null,null,null,null,null,null,null,null,null,null,"1559 / 1046 - 1575 / 1082",null,null,null,"Pays_Plan31","Pays_Plan32",null,"BacAc","Bac acier","Steel Decks","Wellblech"]
["Etrier Double Renforcé H19 ALU","EDH192014ALU",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pays_Plan41","Pays_Plan42",null,"Fibro","Fibrociment","Fibro-Cement","Faserzement"]
["Etrier Double Renforcé H21 ALU","EDH212014ALU",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pays_Plan51","Pays_Plan52",null,"InclT","Inclinaison de toiture","Roof Slope","Dachneigung"]
["Etrier Double Renforcé H23 ALU","EDH232014ALU",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pays_Plan61","Pays_Plan62",null,"RacFait","Raccord faitage","Ridge connection","Firstanbindung"]
["Etrier Double Renforcé H27 ALU","EDH272014ALU",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"None1","Aucun","None","Kein"]
["Etrier Double Renforcé H31 ALU","EDH312014ALU",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AberFait","Abergement de faitage","Top Centre Flashing","Firstverblechung"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RacEgout","Raccord à l'égout","Connection to Sewer","Abwasseranschluss"]
["Liste de références \"Etriers simples\"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PowerMod","Puissance module","Module Power","Modulleistung"]
["Etrier Simple Renforcé H16 NOIR","ESH162014N ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AberLat","Abergements latéraux","Lateral Flashing","Seitliche Verblechung"]
["Etrier Simple Renforcé H19 NOIR","ESH192014N ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NbrEtrier","Nombre d'étriers par module","Number of Clamps per modules","Anzahl Klemmen pro Modul"]
["Etrier Simple Renforcé H21 NOIR","ESH212014N ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LargRooflex","Largeur Rooflex","Rooflex Width","Breite ROOFLEX"]
["Etrier Simple Renforcé H23 NOIR","ESH232014N ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Noir","NOIR","BLACK","SCHWARZ"]
["Etrier Simple Renforcé H27 NOIR","ESH272014N ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Red","Rouge","Red","Rot"]
["Etrier Simple Renforcé H31 NOIR","ESH312014N ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RoofDisplay","Afficher le toit","View the Roof","Dach anzeigen"]
["Etrier Simple Renforcé H16 ALU","ESH162014ALU",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Var33","Accueil","Home","Startseite"]
["Etrier Simple Renforcé H19 ALU","ESH192014ALU",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CalInstr","Colorier le toit (surface encadrée ci-dessous) à l'aide de la souris, en selectionnant les cellules/cases correspondant aux modules, pour créer le champ PV souhaité.","Color the roof (framed surface below) using the mouse, by selecting the cells / boxes corresponding to the modules, to create the desired PV Plant.","das Dach (untenstehende, gerahmte Fläche) mit Hilfe der Maus markieren und über das Auswählen der einzelnen Zellen das entsprechende PV-Modulfeld erstellen"]
["Etrier Simple Renforcé H21 ALU","ESH212014ALU",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NbrRows","Nombres de lignes","Number of Lines","Anzahl der Zeilen"]
["Etrier Simple Renforcé H23 ALU","ESH232014ALU",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NbrCol","Nombres de colonnes","Number of Columns","Anzahl der Spalten"]
["Etrier Simple Renforcé H27 ALU","ESH272014ALU",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NbrMod","Nombres modules","Number of Modules","Anzahl der Module"]
["Etrier Simple Renforcé H31 ALU","ESH312014ALU",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ernergy","Energie","Energie","Energie"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Var39","Effacer champ PV","Erase PV Plant","Modulfeld löschen"]
["http://www.gseintegration.com/InRoof.html",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Var40","Bon de commande","Purchase Order","Bestellformular"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NbrPiece","Nombre de pièces","Number of Pieces","Anzahl der Zimmer"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PlakGSEPays","Plaques GSE Paysage","GSE Frames Landscape","GSE-Wanne Querformat"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PlakGSEPort","Plaques GSE Portrait","GSE Frames Portrait","GSE-Wanne Hochkant"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AberLatUniv","Abergement latéral Universel","Universal Lateral Flashing","Seitliche, Verblechung Universal"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AberFaitD","Abergement Faîtage Droit","Top Right Corner Flashing","Eckverblechung rechts"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AberFaitG","Abergement faîtage Gauche","Top Left Corner Flashing","Eckverblechung links"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AberFaitC","Abergement Faîtage central","Top Centre Flashing","First-Hauptverblechung"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Corniere","Corniere ( pour Faîtage central)","Corner Piece (To Join Module to Top Centre Flashings)","Verbindungsstück (zur Befestigung der zentralen Verblechung)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rivets","Rivets Pop (4 rivets de fixation par corniere de faîtage)","Pop Rivet (4-Fixations Rivet for Top Centre Flashing)","Pop-Niete (Halter für Verbindungsstücke)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VisRondP","Vis + rondelle (6 par plaque) ALU","Selt-Trapping Screw + GSE Washer Silver ( 6 per Frame)","Schraube + GSE Unterlegscheibe (6 pro Platte) ALU"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VisRondE","Vis + rondelle pour fixation des étriers","Selt-Trapping Screw + GSE Washer Black to fix Clamp","Schraube + Unterlegscheibe zur Befestigung der Modulklemme"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Joints","Joints EPDM Cellulaire ","Cale EPDM Cell","EPDM-Dichtung CELL klebend"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EtrDbl","Etrier Double Renforcé","Reinforced Double Clamp","Verstärkte Mittel-Klemme"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EtrSpl","Etrier Simple renforcé","Reinforced Single Clamp","Verstärkte Rand-Klemme"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Grappe","Grappe de 4 Cales de renfort G et D pour étriers simples","Batch of 4 Reinforcement GSE Wedges L and R for Single Clamps","Cluster von 4 Randverstärkungen L und R für Rand-Klemme"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Crochet","Crochets fixation abergements","GSE Flashing Hook","Hafte zur Befestigung der Verblechung"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Option","Options","Options","Optionen"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rooflex","Bande d'étanchéité ROOFLEX (Rouleau de 5 m)","ROOFLEX Waterproof Strip (5 m roll)","ROOFLEX Dichtungband (5 m-Rolle)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EcranToit","Ecran de sous toiture (Rouleau de 75 m²)","Roof-Underlay Screen (75 m² roll)","Unterspannbahn (75 m²-Rolle)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JointImpr","Joint pré-contraint - 20 x 40 mm (Rouleau de 5.5 m)","Pre-Compressed Seal Roll - 20 x 40 mm (5.5 m roll)","Vorkomprimiertes Dichtungsband - 20 x 40 mm (5.5 m-Rolle)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DimChamp","Taille du champ PV","Size of the PV Plant","Größe des Modulfeldes"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HautCmpARE","Hauteur (avec Rooflex en partie basse)","Height (with Low Rooflex)","Höhe (mit Rooflex an der Unterseite)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LargCmpAAL","Largeur (avec abergements latéraux)","Width (with Lateral Flashing)","Breite (mit seitlicher Verblechung)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Coord","Coordonnées","Contact Details","Kontaktdaten"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DateExp","Date d'expedition souhaitée","Desired Shipping Date","Gewünschtes Versanddatum"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Adr","Adresse / Contact / Commentaires","Address / Contact / Comments","Adresse / Kontakt / Kommentare"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ScrolTitle","(Dimensions : Toit, Module PV & Plaque GSE)","(Dimensions: Roof, PV Module & GSE Plate)","(Größe: Dach, PV-Modul & GSE-Wanne)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Toit","Toit","Roof","Dach"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ModPV","Module PV","PV Module","PV-Modul"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Adj","Ajustement","Adjustment","Anpassung"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PlakGSE","Plaque GSE","GSE Plate","GSE-Wanne"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ref","Références","References","Referenzen"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Den","Dénomination","Denomination","Bezeichnung"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CalcRampTitle","Calculer le Rampant du toit","Calculate the Roof Rake","Berechnung der Länge der Dachschräge"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LargMsn","Largeur de la maison (m)","Width of the house (m)","Breite des Hauses (m)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NbrPans","Nombre de Pans","Number of Pans","Anzahl der Dachschrägen"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Calculer","Calculer","Compute","Berechnen"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Annuler","Annuler","Cancel","Abbrechen"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CalcRampMsg1","Les champs suivants doivent contenir une valeur numérique positive non nulle: 'Inclinaison toiture' et 'Largeur de la maison'.","\nThe following fields must contain a non-zero positive numeric value: 'Roof Slope' and 'Width of the House'.\n","Die folgenden Felder müssen einen positiven numerischen Wert ungleich Null enthalten: \"Dachneigung\" und \"Breite des Hauses\"."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CalcRampMsg2","Veuillez vérifier les valeurs de ces champs puis lancez de nouveau le calcul du Rampant.","Please check the values ​​of these fileds then run the Roof Rake calculation again.","Bitte überprüfen Sie die Werte dieser Felder und führen Sie die Berechnung der Länge der Dachschräge erneut aus."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DftRefCmpPV","Champ PV 1","PV Plant 1","PV-Modulfeld 1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CalcRampLink","Cliquez ici pour calculer le Rampant !","Click here to calculate the Roof Rake !","Klicken Sie hier, um die Länge der Dachschräge zu berechnen !"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"None2","Aucune","None","keine Angabe"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ColorAber","Couleur abergement","Flashing color","Farbe der Verblechung"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Yes","Oui","Yes","Ja"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","Non","No","Nein"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ErrInfoMsg1","Ce champ doit contenir un nombre entre","This field must contain a number between","Dieses Feld muss eine Zahl enthalten zwischen"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"And","et","and","und"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LongToit","Longueur du toit","Roof length","Dachlänge"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RampToit","Rampant du toit","Roof Rake","Länge der Dachschräge"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HautModPVPo","Hauteur du module PV portrait","PV Portrait Module Height","Modulhöhe bei Hochkantmontage"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HautModPVPa","Hauteur du module PV paysage","PV Landscape Module Height","Modulhöhe bei Querformatmontage"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LargModPVPo","Largeur du module PV portrait","PV Portrait Module Width","Modulbreite bei Hochkantmontage"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LargModPVPa","Largeur du module PV paysage","PV Landscape Module Width","Modulbreite bei Querformatmontage"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ErrInfoMsg2","Le champ PV à créer doit avoir une référence d'au moins 6 caratères alphanumérique.","The PV plant to be created must have a reference of at least 6 alphanumeric characters.","Das zu erstellende PV-Feld muss eine Referenzangabe von mindestens 6 alphanumerischen Zeichen haben."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ErrInfoMsg3","Dans le cadre des évaluations techniques du système, l'étanchéité est garantie sur des pentes comprises entre 12° et 50°.","As part of the technical evaluations of the system, waterproofing is guaranteed on slopes between 12° and 50°.","Im Rahmen der technischen Bewertungen des Systems ist die Wasserdichtheit bei Dachneigungen zwischen 12 ° und 50 ° garantiert."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ErrInfoMsg4","En dessous et en dessus de ces pentes, bien contrôler l'étanchéité et la méthode de pose de l'installation.","Below and above these slopes, check the tightness and installation method of the plant.","Unterhalb und oberhalb dieser Dachneigungen sind Dichtheit und Installationsart der Anlage gesondert zu prüfen."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ErrInfoMsg5","L'utilisation des abergements de faitage n'est conseillée que sur des pentes supérieures à 17°.","The use of shading is recommended only on slopes greater than 17°.","Die Verwendung der Firstverblechung wird nur bei Neigungen empfohlen, die größer als 17 ° sind."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ErrInfoMsg6","En dessous de cette pente, bien se référer à la notice d'installation en ligne: ","Below this slope, refer to the online installation instructions: ","Unterhalb dieser Dachneigung finden Sie gesonderte Hinweise in den Online-Installationsanweisungen: "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ErrInfoMsg7","Aucune plaque GSE correspondante n'a été trouvée !","No corresponding GSE plate was found !","Es wurde keine passende GSE-Wanne gefunden!"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ErrInfoMsg8","Modifiez les dimensions du module PV pour trouver une plaque GSE correspondante.","Change the dimensions of the PV module to find a corresponding GSE plate.","Ändern Sie die Abmessungen des PV-Moduls, um eine passende GSE-Wanne zu finden."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ErrInfoMsg9","Aucune référence du champ PV n'a été renseignée !","No reference of the PV plant has been entered !","Es wurde keine Referenz der PV-Anlage eingegeben!"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ErrInfoMsg10","Reseignez-en un.","Fill in one.","Bitte einmal ausfüllen."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Date","Date","Date","Datum"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Total","Total","Total","Gesamt"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PlanLat","Plan de lattage indisponible","Layout plan unavailable","Lattenplan nicht verfügbar"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Roul","Rouleau(x)","Roll(s)","Rolle(n)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HautCmpSRFRE","Hauteur (sans Raccord faîtage et Raccord à l'égout)","Height (without Ridge connection and Connection to Sewer)","Höhe (ohne Firstanbindung und Abwasseranschluss)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LargCmpSAL","Largeur (sans abergements latéraux)","Width (without Lateral Flashing)","Breite (ohne seitliche Verblechung)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Remise","Remise","Discount","Rabatt"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RemiseQuest","Avez-vous une remise ?","Do you have a discount ?","Haben Sie Rabatt?"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ErrInfoMsg11","La valeur de la remise saisie n'est pas correcte.","The discount value entered is not correct.","Der Wert des eingegebenen Rabattes ist nicht korrekt."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HautCmpARF","Hauteur (avec Raccord faîtage)","Height (with Ridge connection)","Höhe (mit Firstanbindung)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HautCmpARFRE","Hauteur (avec Raccord faîtage et Raccord à l'égout)","Height (with Ridge connection and Connection to Sewer)","Höhe (mit Firstanbindung und Abwasseranschluss)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PUHT","P.U. (HT)","Unit Price (Excl Tax)","Pro Einheit (zzgl. MwSt.)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AberFaitJonc","Abergement Faîtage Jonction","Junction For Top Flashing","Verbindungsblech Firstverblechung"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PUREM","P.U. REMISÉ ","Unit Price Discounted","Pro Einheit Diskontiert"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Portrait","Portrait","Portrait","Hochkant"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Paysage","Paysage","Landscape","Querformat"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NotePriceOpt","NB : Prix disponible auprès de votre interlocuteur habituel.","NB: Price available from your usual contact.","NB: Preis verfügbar von Ihrem üblichen Kontakt."]

{"sheet":"Schémas","index":4,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"1 m"]
[null,"1 m"]